Back to main Back to Kenwood/Trio Next HF and more Last modified 2009-10-20

### Kenwood TS-450S ##### SPECIFICATIONS
Type: | Amateur HF transceiver
Frequency range: | TX: 10-160 m + WARC RX: 0.5-30 MHz
Mode: | AM/FM/SSB/CW
RF Power output: | Max 100 W
Receiver system: | N/A
Sensitivity: | N/A
Selectivity: | N/A
Image rejection: | N/A
Voltage: | 13.8 VDC
Current drain: | RX: ? A TX: Max 20 A
Impedance: | 50 ohms, SO-239
Dimensions (W*H*D): | 270*96*305 mm
Weight: | 7.5 Kg
Manufactured: | 198x-199x (Discontinued)
Other: |
Related documents: |
Modifications: |